(kicad_pcb (version 20171130) (host pcbnew 5.1.9+dfsg1-1+deb11u1)

  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 115)
    (zones 0)
    (modules 31)
    (nets 21)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 2)
    (via_drill 1)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFAFF3F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C2-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 +5V)
  (net 5 "Net-(C4-Pad1)")
  (net 6 +24V)
  (net 7 GNDPWR)
  (net 8 "Net-(J3-Pad2)")
  (net 9 "Net-(Q1-Pad1)")
  (net 10 "Net-(R1-Pad1)")
  (net 11 "Net-(R3-Pad1)")
  (net 12 "Net-(R10-Pad2)")
  (net 13 VT-read)
  (net 14 VT-max)
  (net 15 VT-set)
  (net 16 VT-min)
  (net 17 "Net-(J4-Pad2)")
  (net 18 "Net-(R7-Pad1)")
  (net 19 "Net-(R11-Pad2)")
  (net 20 "Net-(R13-Pad1)")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 1)
    (via_dia 2)
    (via_drill 1)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +24V)
    (add_net +5V)
    (add_net GND)
    (add_net GNDPWR)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net VT-max)
    (add_net VT-min)
    (add_net VT-read)
    (add_net VT-set)
  )

  (module Potentiometer_THT:Potentiometer_Piher_PT-10-V10_Vertical (layer F.Cu) (tedit 5A3D4993) (tstamp 637056B1)
    (at 165.21 60.88 90)
    (descr "Potentiometer, vertical, Piher PT-10-V10, http://www.piher-nacesa.com/pdf/12-PT10v03.pdf")
    (tags "Potentiometer vertical Piher PT-10-V10")
    (path /636B2082)
    (fp_text reference RV2 (at 5 -9.05 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 2k5 (at 5 -0.11 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 5 -2.65) (end 10.15 -2.65) (layer F.Fab) (width 0.1))
    (fp_circle (center 5 -2.65) (end 6.5 -2.65) (layer F.Fab) (width 0.1))
    (fp_line (start -1.45 -8.05) (end -1.45 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 2.75) (end 11.45 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.45 2.75) (end 11.45 -8.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.45 -8.05) (end -1.45 -8.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.05 -2.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 5 -2.65) (end 1.209 1.011) (angle -47) (layer F.SilkS) (width 0.12))
    (fp_arc (start 5 -2.65) (end -0.174 -3.656) (angle -25) (layer F.SilkS) (width 0.12))
    (fp_arc (start 5 -2.65) (end 10.114 -3.924) (angle -126) (layer F.SilkS) (width 0.12))
    (fp_arc (start 5 -2.65) (end 5 2.62) (angle -73) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 2 thru_hole circle (at 10 -2.5 90) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad1)"))
    (pad 3 thru_hole circle (at 0 -5 90) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Piher_PT-10-V10_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Potentiometer_THT:Potentiometer_Piher_PT-10-V10_Vertical (layer F.Cu) (tedit 5A3D4993) (tstamp 6370569F)
    (at 165.21 48.18 90)
    (descr "Potentiometer, vertical, Piher PT-10-V10, http://www.piher-nacesa.com/pdf/12-PT10v03.pdf")
    (tags "Potentiometer vertical Piher PT-10-V10")
    (path /636DDBEF)
    (fp_text reference RV1 (at 5 -9.05 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 5 -0.11 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 5 -2.65) (end 10.15 -2.65) (layer F.Fab) (width 0.1))
    (fp_circle (center 5 -2.65) (end 6.5 -2.65) (layer F.Fab) (width 0.1))
    (fp_line (start -1.45 -8.05) (end -1.45 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 2.75) (end 11.45 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.45 2.75) (end 11.45 -8.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.45 -8.05) (end -1.45 -8.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.05 -2.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 5 -2.65) (end 1.209 1.011) (angle -47) (layer F.SilkS) (width 0.12))
    (fp_arc (start 5 -2.65) (end -0.174 -3.656) (angle -25) (layer F.SilkS) (width 0.12))
    (fp_arc (start 5 -2.65) (end 10.114 -3.924) (angle -126) (layer F.SilkS) (width 0.12))
    (fp_arc (start 5 -2.65) (end 5 2.62) (angle -73) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 2 thru_hole circle (at 10 -2.5 90) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad1)"))
    (pad 3 thru_hole circle (at 0 -5 90) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Piher_PT-10-V10_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 5AE50EF0) (tstamp 637050F2)
    (at 177.88 55.88)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor")
    (path /6375440E)
    (fp_text reference C2 (at 2.5 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 2.46 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.1 -1.25) (end -1.1 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.1 1.25) (end 6.1 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 1.25) (end 6.1 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 -1.25) (end -1.1 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.22 -1.37) (end 6.22 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.22 1.37) (end 6.22 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.22 -1.37) (end -1.22 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.22 -1.37) (end 6.22 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.35 -1.5) (end -1.35 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 1.5) (end 6.35 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.35 1.5) (end 6.35 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.35 -1.5) (end -1.35 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 5AE50EF0) (tstamp 637050DF)
    (at 175.34 73.66)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor")
    (path /6372F288)
    (fp_text reference C1 (at 2.5 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.1 -1.25) (end -1.1 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.1 1.25) (end 6.1 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 1.25) (end 6.1 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.1 -1.25) (end -1.1 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.22 -1.37) (end 6.22 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.22 1.37) (end 6.22 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.22 -1.37) (end -1.22 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.22 -1.37) (end 6.22 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.35 -1.5) (end -1.35 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 1.5) (end 6.35 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.35 1.5) (end 6.35 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.35 -1.5) (end -1.35 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 VT-read))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D) (tstamp 6370551D)
    (at 210.82 55.88 270)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (path /636B5D9F)
    (fp_text reference Q1 (at 2.54 -4.27 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "BUZ11, IRFZ44N, etc." (at 2.54 -7.62 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.79 -3.4) (end -2.71 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.79 1.51) (end 7.79 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.71 1.51) (end 7.79 1.51) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.71 -3.4) (end -2.71 1.51) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.391 -3.27) (end 4.391 -1.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.69 -3.27) (end 0.69 -1.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 -1.76) (end 7.66 -1.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.66 -3.27) (end 7.66 1.371) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 -3.27) (end -2.58 1.371) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 1.371) (end 7.66 1.371) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 -3.27) (end 7.66 -3.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.39 -3.15) (end 4.39 -1.88) (layer F.Fab) (width 0.1))
    (fp_line (start 0.69 -3.15) (end 0.69 -1.88) (layer F.Fab) (width 0.1))
    (fp_line (start -2.46 -1.88) (end 7.54 -1.88) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 -3.15) (end -2.46 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 1.25) (end 7.54 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.46 1.25) (end 7.54 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -2.46 -3.15) (end -2.46 1.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 2.54 -4.27 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 GNDPWR))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_D13.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1) (tstamp 6370540E)
    (at 203.2 71.12 180)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=13mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 13mm Electrolytic Capacitor")
    (path /636B08FC)
    (fp_text reference C6 (at 2.5 -7.75) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "220µ 35V" (at 2.5 2.54) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.934569 -4.365) (end -3.934569 -3.065) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.584569 -3.715) (end -3.284569 -3.715) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.101 -0.475) (end 9.101 0.475) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.061 -0.85) (end 9.061 0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.021 -1.107) (end 9.021 1.107) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.981 -1.315) (end 8.981 1.315) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.941 -1.494) (end 8.941 1.494) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.901 -1.653) (end 8.901 1.653) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.861 -1.798) (end 8.861 1.798) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.821 -1.931) (end 8.821 1.931) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.781 -2.055) (end 8.781 2.055) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.741 -2.171) (end 8.741 2.171) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.701 -2.281) (end 8.701 2.281) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.661 -2.385) (end 8.661 2.385) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.621 -2.484) (end 8.621 2.484) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.581 -2.579) (end 8.581 2.579) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.541 -2.67) (end 8.541 2.67) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.501 -2.758) (end 8.501 2.758) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.461 -2.842) (end 8.461 2.842) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.421 -2.923) (end 8.421 2.923) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.381 -3.002) (end 8.381 3.002) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.341 -3.078) (end 8.341 3.078) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.301 -3.152) (end 8.301 3.152) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.261 -3.223) (end 8.261 3.223) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.221 -3.293) (end 8.221 3.293) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.181 -3.361) (end 8.181 3.361) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.141 -3.427) (end 8.141 3.427) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.101 -3.491) (end 8.101 3.491) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.061 -3.554) (end 8.061 3.554) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.021 -3.615) (end 8.021 3.615) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.981 -3.675) (end 7.981 3.675) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.941 -3.733) (end 7.941 3.733) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.901 -3.79) (end 7.901 3.79) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.861 -3.846) (end 7.861 3.846) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.821 -3.9) (end 7.821 3.9) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.781 -3.954) (end 7.781 3.954) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.741 -4.006) (end 7.741 4.006) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.701 -4.057) (end 7.701 4.057) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.661 -4.108) (end 7.661 4.108) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.621 -4.157) (end 7.621 4.157) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.581 -4.205) (end 7.581 4.205) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.541 -4.253) (end 7.541 4.253) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.501 -4.299) (end 7.501 4.299) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.461 -4.345) (end 7.461 4.345) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.421 -4.39) (end 7.421 4.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.381 -4.434) (end 7.381 4.434) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.341 -4.477) (end 7.341 4.477) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.301 -4.519) (end 7.301 4.519) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.261 -4.561) (end 7.261 4.561) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.221 -4.602) (end 7.221 4.602) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.181 -4.643) (end 7.181 4.643) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.141 -4.682) (end 7.141 4.682) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.101 -4.721) (end 7.101 4.721) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.061 -4.76) (end 7.061 4.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.021 -4.797) (end 7.021 4.797) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.981 -4.834) (end 6.981 4.834) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.941 -4.871) (end 6.941 4.871) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.901 -4.907) (end 6.901 4.907) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.861 -4.942) (end 6.861 4.942) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.821 -4.977) (end 6.821 4.977) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.781 -5.011) (end 6.781 5.011) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.741 -5.044) (end 6.741 5.044) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.701 -5.078) (end 6.701 5.078) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.661 -5.11) (end 6.661 5.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.621 -5.142) (end 6.621 5.142) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.581 -5.174) (end 6.581 5.174) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.541 -5.205) (end 6.541 5.205) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.501 -5.235) (end 6.501 5.235) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.461 -5.265) (end 6.461 5.265) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.421 1.44) (end 6.421 5.295) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.421 -5.295) (end 6.421 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.381 1.44) (end 6.381 5.324) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.381 -5.324) (end 6.381 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.341 1.44) (end 6.341 5.353) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.341 -5.353) (end 6.341 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.301 1.44) (end 6.301 5.381) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.301 -5.381) (end 6.301 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.261 1.44) (end 6.261 5.409) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.261 -5.409) (end 6.261 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.221 1.44) (end 6.221 5.436) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.221 -5.436) (end 6.221 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.181 1.44) (end 6.181 5.463) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.181 -5.463) (end 6.181 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.141 1.44) (end 6.141 5.49) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.141 -5.49) (end 6.141 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.101 1.44) (end 6.101 5.516) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.101 -5.516) (end 6.101 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.061 1.44) (end 6.061 5.542) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.061 -5.542) (end 6.061 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.021 1.44) (end 6.021 5.567) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.021 -5.567) (end 6.021 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.981 1.44) (end 5.981 5.592) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.981 -5.592) (end 5.981 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.941 1.44) (end 5.941 5.617) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.941 -5.617) (end 5.941 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.901 1.44) (end 5.901 5.641) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.901 -5.641) (end 5.901 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.861 1.44) (end 5.861 5.664) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.861 -5.664) (end 5.861 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.821 1.44) (end 5.821 5.688) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.821 -5.688) (end 5.821 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.781 1.44) (end 5.781 5.711) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.781 -5.711) (end 5.781 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.741 1.44) (end 5.741 5.733) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.741 -5.733) (end 5.741 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.701 1.44) (end 5.701 5.756) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.701 -5.756) (end 5.701 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.661 1.44) (end 5.661 5.778) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.661 -5.778) (end 5.661 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.621 1.44) (end 5.621 5.799) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.621 -5.799) (end 5.621 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.581 1.44) (end 5.581 5.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.581 -5.82) (end 5.581 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.541 1.44) (end 5.541 5.841) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.541 -5.841) (end 5.541 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.501 1.44) (end 5.501 5.862) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.501 -5.862) (end 5.501 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.461 1.44) (end 5.461 5.882) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.461 -5.882) (end 5.461 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.421 1.44) (end 5.421 5.902) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.421 -5.902) (end 5.421 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.381 1.44) (end 5.381 5.921) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.381 -5.921) (end 5.381 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.341 1.44) (end 5.341 5.94) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.341 -5.94) (end 5.341 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.301 1.44) (end 5.301 5.959) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.301 -5.959) (end 5.301 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.261 1.44) (end 5.261 5.978) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.261 -5.978) (end 5.261 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.221 1.44) (end 5.221 5.996) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.221 -5.996) (end 5.221 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.181 1.44) (end 5.181 6.014) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.181 -6.014) (end 5.181 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.141 1.44) (end 5.141 6.031) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.141 -6.031) (end 5.141 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.101 1.44) (end 5.101 6.049) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.101 -6.049) (end 5.101 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.061 1.44) (end 5.061 6.065) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.061 -6.065) (end 5.061 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.021 1.44) (end 5.021 6.082) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.021 -6.082) (end 5.021 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.981 1.44) (end 4.981 6.098) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.981 -6.098) (end 4.981 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.941 1.44) (end 4.941 6.114) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.941 -6.114) (end 4.941 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.901 1.44) (end 4.901 6.13) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.901 -6.13) (end 4.901 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.861 1.44) (end 4.861 6.146) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.861 -6.146) (end 4.861 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.821 1.44) (end 4.821 6.161) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.821 -6.161) (end 4.821 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.781 1.44) (end 4.781 6.175) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.781 -6.175) (end 4.781 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.741 1.44) (end 4.741 6.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.741 -6.19) (end 4.741 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.701 1.44) (end 4.701 6.204) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.701 -6.204) (end 4.701 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.661 1.44) (end 4.661 6.218) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.661 -6.218) (end 4.661 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.621 1.44) (end 4.621 6.232) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.621 -6.232) (end 4.621 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.581 1.44) (end 4.581 6.245) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.581 -6.245) (end 4.581 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.541 1.44) (end 4.541 6.258) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.541 -6.258) (end 4.541 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.501 1.44) (end 4.501 6.271) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.501 -6.271) (end 4.501 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.461 1.44) (end 4.461 6.284) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.461 -6.284) (end 4.461 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.421 1.44) (end 4.421 6.296) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.421 -6.296) (end 4.421 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.381 1.44) (end 4.381 6.308) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.381 -6.308) (end 4.381 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.341 1.44) (end 4.341 6.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.341 -6.32) (end 4.341 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.301 1.44) (end 4.301 6.331) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.301 -6.331) (end 4.301 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.261 1.44) (end 4.261 6.342) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.261 -6.342) (end 4.261 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.221 1.44) (end 4.221 6.353) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.221 -6.353) (end 4.221 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.181 1.44) (end 4.181 6.364) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.181 -6.364) (end 4.181 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.141 1.44) (end 4.141 6.374) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.141 -6.374) (end 4.141 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.101 1.44) (end 4.101 6.384) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.101 -6.384) (end 4.101 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.061 1.44) (end 4.061 6.394) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.061 -6.394) (end 4.061 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.021 1.44) (end 4.021 6.404) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.021 -6.404) (end 4.021 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.981 1.44) (end 3.981 6.413) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.981 -6.413) (end 3.981 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.941 1.44) (end 3.941 6.422) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.941 -6.422) (end 3.941 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.901 1.44) (end 3.901 6.431) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.901 -6.431) (end 3.901 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.861 1.44) (end 3.861 6.439) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.861 -6.439) (end 3.861 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.821 1.44) (end 3.821 6.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.821 -6.448) (end 3.821 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.781 1.44) (end 3.781 6.456) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.781 -6.456) (end 3.781 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.741 1.44) (end 3.741 6.463) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.741 -6.463) (end 3.741 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.701 1.44) (end 3.701 6.471) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.701 -6.471) (end 3.701 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.661 1.44) (end 3.661 6.478) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.661 -6.478) (end 3.661 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.621 1.44) (end 3.621 6.485) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.621 -6.485) (end 3.621 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.581 1.44) (end 3.581 6.492) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.581 -6.492) (end 3.581 -1.44) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.541 -6.498) (end 3.541 6.498) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.501 -6.505) (end 3.501 6.505) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.461 -6.511) (end 3.461 6.511) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.421 -6.516) (end 3.421 6.516) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.381 -6.522) (end 3.381 6.522) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.341 -6.527) (end 3.341 6.527) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.301 -6.532) (end 3.301 6.532) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.261 -6.537) (end 3.261 6.537) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.221 -6.541) (end 3.221 6.541) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.18 -6.545) (end 3.18 6.545) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.14 -6.549) (end 3.14 6.549) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.1 -6.553) (end 3.1 6.553) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.06 -6.557) (end 3.06 6.557) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.02 -6.56) (end 3.02 6.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.98 -6.563) (end 2.98 6.563) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.94 -6.566) (end 2.94 6.566) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.9 -6.568) (end 2.9 6.568) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.86 -6.571) (end 2.86 6.571) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.82 -6.573) (end 2.82 6.573) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.78 -6.575) (end 2.78 6.575) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.74 -6.576) (end 2.74 6.576) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.7 -6.577) (end 2.7 6.577) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.66 -6.579) (end 2.66 6.579) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.62 -6.579) (end 2.62 6.579) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.58 -6.58) (end 2.58 6.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.54 -6.58) (end 2.54 6.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.5 -6.58) (end 2.5 6.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.432015 -3.4975) (end -2.432015 -2.1975) (layer F.Fab) (width 0.1))
    (fp_line (start -3.082015 -2.8475) (end -1.782015 -2.8475) (layer F.Fab) (width 0.1))
    (fp_circle (center 2.5 0) (end 9.25 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.5 0) (end 9.12 0) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.5 0) (end 9 0) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole circle (at 5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 GNDPWR))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 +24V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D13.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P5.08mm_Vertical (layer F.Cu) (tedit 5AE5139B) (tstamp 637055EC)
    (at 187.96 43.18 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=5.08mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 5.08mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /6394DC28)
    (fp_text reference R10 (at 2.54 -2.37) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 47k (at 2.54 5.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 6.13 -1.5) (end -1.5 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.13 1.5) (end 6.13 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 1.5) (end 6.13 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 -1.5) (end -1.5 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.37 0) (end 3.98 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 0) (end 5.08 0) (layer F.Fab) (width 0.1))
    (fp_circle (center 0 0) (end 1.37 0) (layer F.SilkS) (width 0.12))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 2.54 -2.37) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R10-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5) (tstamp 637056D5)
    (at 180.34 53.34 90)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (path /636ADFA1)
    (fp_text reference U1 (at 3.81 -2.33 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TL494 (at 3.81 12.7 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.7 -1.55) (end -1.1 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 19.3) (end 8.7 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 19.3) (end 8.7 19.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 -1.55) (end -1.1 19.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 19.11) (end 6.46 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 19.11) (end 6.46 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -1.33) (end 1.16 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 19.05) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 19.05) (end 0.635 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 3.81 8.89 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (pad 16 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R13-Pad1)"))
    (pad 15 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R10-Pad2)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(R11-Pad2)"))
    (pad 13 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 12 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +24V))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R13-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad2)"))
    (pad 10 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GNDPWR))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 9 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GNDPWR))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 6370568D)
    (at 185.42 66.04 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /63A4DD5E)
    (fp_text reference R9 (at 5.08 -2.37 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1M (at 5.08 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.12 0) (end 8.35 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 0) (end 1.81 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.16 0) (end 8.23 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.93 0) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 6370C797)
    (at 210.82 76.2 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /638A65A0)
    (fp_text reference R16 (at 5.08 -2.37 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 2k2 (at 5.08 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.12 0) (end 8.35 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 0) (end 1.81 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.16 0) (end 8.23 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.93 0) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(J4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 6370565F)
    (at 208.28 55.88 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /6389A789)
    (fp_text reference R15 (at 5.08 -2.37) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220 (at 5.08 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.12 0) (end 8.35 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 0) (end 1.81 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.16 0) (end 8.23 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.93 0) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 5.08 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R13-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 63705648)
    (at 208.28 58.42 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /638A5D99)
    (fp_text reference R14 (at 5.08 -2.37) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 5.08 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.12 0) (end 8.35 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 0) (end 1.81 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.16 0) (end 8.23 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.93 0) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 5.08 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R13-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GNDPWR))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 63705631)
    (at 200.66 53.34)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /638A5666)
    (fp_text reference R13 (at 5.08 -2.37) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 5.08 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.12 0) (end 8.35 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 0) (end 1.81 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.16 0) (end 8.23 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.93 0) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 5.08 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +24V))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R13-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 6370561A)
    (at 195.58 66.04 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /63A39833)
    (fp_text reference R12 (at 5.08 -2.37 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0 (at 5.08 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.12 0) (end 8.35 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 0) (end 1.81 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.16 0) (end 8.23 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.93 0) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GNDPWR))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 63705603)
    (at 193.04 66.04 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /6394E5C1)
    (fp_text reference R11 (at 5.08 -2.37 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220k (at 5.08 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.12 0) (end 8.35 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 0) (end 1.81 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.16 0) (end 8.23 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.93 0) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(R11-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 6370F975)
    (at 182.88 58.42 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /6375391C)
    (fp_text reference R8 (at 5.08 -2.37) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 120k (at 5.08 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.12 0) (end 8.35 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 0) (end 1.81 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.16 0) (end 8.23 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.93 0) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 5.08 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 637055BE)
    (at 172.72 63.5 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /63706911)
    (fp_text reference R7 (at 5.08 -2.37 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4k7 (at 5.08 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.12 0) (end 8.35 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 0) (end 1.81 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.16 0) (end 8.23 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.93 0) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 VT-set))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 637055A7)
    (at 175.26 60.96 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /6372E411)
    (fp_text reference R6 (at 5.08 -2.37 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 5.08 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.12 0) (end 8.35 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 0) (end 1.81 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.16 0) (end 8.23 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.93 0) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 VT-read))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 63705590)
    (at 170.18 60.96 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /636AEC3D)
    (fp_text reference R5 (at 5.08 -2.37 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 5.08 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.12 0) (end 8.35 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 0) (end 1.81 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.16 0) (end 8.23 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.93 0) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 VT-read))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 63705579)
    (at 165.1 66.04 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /636DD49B)
    (fp_text reference R4 (at 5.08 -2.37 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 5.08 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.12 0) (end 8.35 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 0) (end 1.81 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.16 0) (end 8.23 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.93 0) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VT-max))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 63705562)
    (at 167.64 66.04 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /636F957C)
    (fp_text reference R3 (at 5.08 -2.37 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 15k4 (at 5.08 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.12 0) (end 8.35 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 0) (end 1.81 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.16 0) (end 8.23 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.93 0) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VT-max))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 6370554B)
    (at 160.02 66.04 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /636DCA9E)
    (fp_text reference R2 (at 5.08 -2.37 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100 (at 5.08 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.12 0) (end 8.35 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 0) (end 1.81 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.16 0) (end 8.23 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.93 0) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 VT-min))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 63705534)
    (at 157.48 66.04 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /636EF701)
    (fp_text reference R1 (at 5.08 -2.37 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 2k7 (at 5.08 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.12 0) (end 8.35 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 0) (end 1.81 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.16 0) (end 8.23 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.93 0) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 VT-min))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_2-G-5,08_1x02_P5.08mm_Vertical (layer F.Cu) (tedit 5B785047) (tstamp 63705503)
    (at 185.42 83.82)
    (descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/2-G-5,08; number of pins: 02; pin pitch: 5.08mm; Vertical || order number: 1755736 12A || order number: 1924305 16A (HC)")
    (tags "phoenix_contact connector MSTBVA_01x02_G_5.08mm")
    (path /63895CDD)
    (fp_text reference J5 (at 2.54 -6) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 24VDC (at 2.54 7.62) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.5 -3.55) (end 0.5 -3.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0 -2.55) (end -0.5 -3.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 -3.55) (end 0 -2.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.3 -5.71) (end 0.3 -5.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -5.11) (end -0.3 -5.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.3 -5.71) (end 0 -5.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.12 -5.3) (end -4.04 -5.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.12 4.3) (end 9.12 -5.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.04 4.3) (end 9.12 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.04 -5.3) (end -4.04 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.82 2.2) (end 7.08 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.82 -3.1) (end 7.82 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.74 -3.1) (end 7.82 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.74 2.2) (end -2.74 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2 2.2) (end -2.74 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2 2.2) (end 3.08 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.08 -3.1) (end 4.08 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.08 -4.91) (end 6.08 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.08 -4.91) (end 6.08 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.08 -3.1) (end 4.08 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 -3.1) (end -1 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 -4.91) (end 1 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -4.91) (end 1 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -3.1) (end -1 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 -4.1) (end 4.08 -4.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.73 -4.1) (end 6.19 -4.1) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.65 -4.1) (end -1.11 -4.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.62 -4.8) (end -3.54 -4.8) (layer F.Fab) (width 0.1))
    (fp_line (start 8.62 3.8) (end 8.62 -4.8) (layer F.Fab) (width 0.1))
    (fp_line (start -3.54 3.8) (end 8.62 3.8) (layer F.Fab) (width 0.1))
    (fp_line (start -3.54 -4.8) (end -3.54 3.8) (layer F.Fab) (width 0.1))
    (fp_line (start 8.73 -4.91) (end -3.65 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.73 3.91) (end 8.73 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.65 3.91) (end 8.73 3.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.65 -4.91) (end -3.65 3.91) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 2.54 -4.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 5.08 0.55) (end 3.08 2.2) (angle -100.5) (layer F.SilkS) (width 0.12))
    (fp_arc (start 0 0.55) (end -2 2.2) (angle -100.5) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 6 +24V))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 7 GNDPWR))
    (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_2-G-5,08_1x02_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_2-G-5,08_1x02_P5.08mm_Vertical (layer F.Cu) (tedit 5B785047) (tstamp 637114E8)
    (at 195.58 83.82)
    (descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/2-G-5,08; number of pins: 02; pin pitch: 5.08mm; Vertical || order number: 1755736 12A || order number: 1924305 16A (HC)")
    (tags "phoenix_contact connector MSTBVA_01x02_G_5.08mm")
    (path /6389544B)
    (fp_text reference J4 (at 2.54 -6) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value HEATER (at 2.54 7.62) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.5 -3.55) (end 0.5 -3.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0 -2.55) (end -0.5 -3.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 -3.55) (end 0 -2.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.3 -5.71) (end 0.3 -5.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -5.11) (end -0.3 -5.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.3 -5.71) (end 0 -5.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.12 -5.3) (end -4.04 -5.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.12 4.3) (end 9.12 -5.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.04 4.3) (end 9.12 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.04 -5.3) (end -4.04 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.82 2.2) (end 7.08 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.82 -3.1) (end 7.82 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.74 -3.1) (end 7.82 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.74 2.2) (end -2.74 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2 2.2) (end -2.74 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2 2.2) (end 3.08 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.08 -3.1) (end 4.08 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.08 -4.91) (end 6.08 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.08 -4.91) (end 6.08 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.08 -3.1) (end 4.08 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 -3.1) (end -1 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 -4.91) (end 1 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -4.91) (end 1 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -3.1) (end -1 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 -4.1) (end 4.08 -4.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.73 -4.1) (end 6.19 -4.1) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.65 -4.1) (end -1.11 -4.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.62 -4.8) (end -3.54 -4.8) (layer F.Fab) (width 0.1))
    (fp_line (start 8.62 3.8) (end 8.62 -4.8) (layer F.Fab) (width 0.1))
    (fp_line (start -3.54 3.8) (end 8.62 3.8) (layer F.Fab) (width 0.1))
    (fp_line (start -3.54 -4.8) (end -3.54 3.8) (layer F.Fab) (width 0.1))
    (fp_line (start 8.73 -4.91) (end -3.65 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.73 3.91) (end 8.73 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.65 3.91) (end 8.73 3.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.65 -4.91) (end -3.65 3.91) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 2.54 -4.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 5.08 0.55) (end 3.08 2.2) (angle -100.5) (layer F.SilkS) (width 0.12))
    (fp_arc (start 0 0.55) (end -2 2.2) (angle -100.5) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 17 "Net-(J4-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 6 +24V))
    (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_2-G-5,08_1x02_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_2-G-5,08_1x02_P5.08mm_Vertical (layer F.Cu) (tedit 5B785047) (tstamp 637054AB)
    (at 205.74 83.82)
    (descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/2-G-5,08; number of pins: 02; pin pitch: 5.08mm; Vertical || order number: 1755736 12A || order number: 1924305 16A (HC)")
    (tags "phoenix_contact connector MSTBVA_01x02_G_5.08mm")
    (path /6388C8DD)
    (fp_text reference J3 (at 2.54 -6) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 2.54 7.62) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.5 -3.55) (end 0.5 -3.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0 -2.55) (end -0.5 -3.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 -3.55) (end 0 -2.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.3 -5.71) (end 0.3 -5.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -5.11) (end -0.3 -5.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.3 -5.71) (end 0 -5.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.12 -5.3) (end -4.04 -5.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.12 4.3) (end 9.12 -5.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.04 4.3) (end 9.12 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.04 -5.3) (end -4.04 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.82 2.2) (end 7.08 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.82 -3.1) (end 7.82 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.74 -3.1) (end 7.82 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.74 2.2) (end -2.74 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2 2.2) (end -2.74 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2 2.2) (end 3.08 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.08 -3.1) (end 4.08 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.08 -4.91) (end 6.08 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.08 -4.91) (end 6.08 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.08 -3.1) (end 4.08 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 -3.1) (end -1 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 -4.91) (end 1 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -4.91) (end 1 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -3.1) (end -1 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 -4.1) (end 4.08 -4.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.73 -4.1) (end 6.19 -4.1) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.65 -4.1) (end -1.11 -4.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.62 -4.8) (end -3.54 -4.8) (layer F.Fab) (width 0.1))
    (fp_line (start 8.62 3.8) (end 8.62 -4.8) (layer F.Fab) (width 0.1))
    (fp_line (start -3.54 3.8) (end 8.62 3.8) (layer F.Fab) (width 0.1))
    (fp_line (start -3.54 -4.8) (end -3.54 3.8) (layer F.Fab) (width 0.1))
    (fp_line (start 8.73 -4.91) (end -3.65 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.73 3.91) (end 8.73 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.65 3.91) (end 8.73 3.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.65 -4.91) (end -3.65 3.91) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 2.54 -4.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 5.08 0.55) (end 3.08 2.2) (angle -100.5) (layer F.SilkS) (width 0.12))
    (fp_arc (start 0 0.55) (end -2 2.2) (angle -100.5) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 6 +24V))
    (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_2-G-5,08_1x02_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_3-G-5,08_1x03_P5.08mm_Vertical (layer F.Cu) (tedit 5B785047) (tstamp 6370547F)
    (at 160.02 83.82)
    (descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/3-G-5,08; number of pins: 03; pin pitch: 5.08mm; Vertical || order number: 1755749 12A || order number: 1924318 16A (HC)")
    (tags "phoenix_contact connector MSTBVA_01x03_G_5.08mm")
    (path /636B4520)
    (fp_text reference J2 (at 5.08 -6) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "POT 10kB LIN" (at 5.08 7.62) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.5 -3.55) (end 0.5 -3.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0 -2.55) (end -0.5 -3.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 -3.55) (end 0 -2.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.3 -5.71) (end 0.3 -5.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -5.11) (end -0.3 -5.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.3 -5.71) (end 0 -5.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 14.2 -5.3) (end -4.04 -5.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 14.2 4.3) (end 14.2 -5.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.04 4.3) (end 14.2 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.04 -5.3) (end -4.04 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.9 2.2) (end 12.16 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.9 -3.1) (end 12.9 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.74 -3.1) (end 12.9 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.74 2.2) (end -2.74 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2 2.2) (end -2.74 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.08 2.2) (end 8.16 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2 2.2) (end 3.08 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.16 -3.1) (end 9.16 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.16 -4.91) (end 11.16 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.16 -4.91) (end 11.16 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.16 -3.1) (end 9.16 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.08 -3.1) (end 4.08 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.08 -4.91) (end 6.08 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.08 -4.91) (end 6.08 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.08 -3.1) (end 4.08 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 -3.1) (end -1 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 -4.91) (end 1 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -4.91) (end 1 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -3.1) (end -1 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.08 -4.1) (end 9.16 -4.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 -4.1) (end 4.08 -4.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.81 -4.1) (end 11.27 -4.1) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.65 -4.1) (end -1.11 -4.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.7 -4.8) (end -3.54 -4.8) (layer F.Fab) (width 0.1))
    (fp_line (start 13.7 3.8) (end 13.7 -4.8) (layer F.Fab) (width 0.1))
    (fp_line (start -3.54 3.8) (end 13.7 3.8) (layer F.Fab) (width 0.1))
    (fp_line (start -3.54 -4.8) (end -3.54 3.8) (layer F.Fab) (width 0.1))
    (fp_line (start 13.81 -4.91) (end -3.65 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.81 3.91) (end 13.81 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.65 3.91) (end 13.81 3.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.65 -4.91) (end -3.65 3.91) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 5.08 -4.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 10.16 0.55) (end 8.16 2.2) (angle -100.5) (layer F.SilkS) (width 0.12))
    (fp_arc (start 5.08 0.55) (end 3.08 2.2) (angle -100.5) (layer F.SilkS) (width 0.12))
    (fp_arc (start 0 0.55) (end -2 2.2) (angle -100.5) (layer F.SilkS) (width 0.12))
    (pad 3 thru_hole oval (at 10.16 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 14 VT-max))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 VT-set))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 16 VT-min))
    (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_3-G-5,08_1x03_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_2-G-5,08_1x02_P5.08mm_Vertical (layer F.Cu) (tedit 5B785047) (tstamp 6370544B)
    (at 175.26 83.82)
    (descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/2-G-5,08; number of pins: 02; pin pitch: 5.08mm; Vertical || order number: 1755736 12A || order number: 1924305 16A (HC)")
    (tags "phoenix_contact connector MSTBVA_01x02_G_5.08mm")
    (path /636B3739)
    (fp_text reference J1 (at 2.54 -6) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SENSOR (at 2.54 7.62) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.5 -3.55) (end 0.5 -3.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0 -2.55) (end -0.5 -3.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 -3.55) (end 0 -2.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.3 -5.71) (end 0.3 -5.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -5.11) (end -0.3 -5.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.3 -5.71) (end 0 -5.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.12 -5.3) (end -4.04 -5.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.12 4.3) (end 9.12 -5.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.04 4.3) (end 9.12 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.04 -5.3) (end -4.04 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.82 2.2) (end 7.08 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.82 -3.1) (end 7.82 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.74 -3.1) (end 7.82 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.74 2.2) (end -2.74 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2 2.2) (end -2.74 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 2 2.2) (end 3.08 2.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.08 -3.1) (end 4.08 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.08 -4.91) (end 6.08 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.08 -4.91) (end 6.08 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.08 -3.1) (end 4.08 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 -3.1) (end -1 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 -4.91) (end 1 -3.1) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -4.91) (end 1 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -3.1) (end -1 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 -4.1) (end 4.08 -4.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.73 -4.1) (end 6.19 -4.1) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.65 -4.1) (end -1.11 -4.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.62 -4.8) (end -3.54 -4.8) (layer F.Fab) (width 0.1))
    (fp_line (start 8.62 3.8) (end 8.62 -4.8) (layer F.Fab) (width 0.1))
    (fp_line (start -3.54 3.8) (end 8.62 3.8) (layer F.Fab) (width 0.1))
    (fp_line (start -3.54 -4.8) (end -3.54 3.8) (layer F.Fab) (width 0.1))
    (fp_line (start 8.73 -4.91) (end -3.65 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.73 3.91) (end 8.73 -4.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.65 3.91) (end 8.73 3.91) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.65 -4.91) (end -3.65 3.91) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 2.54 -4.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 5.08 0.55) (end 3.08 2.2) (angle -100.5) (layer F.SilkS) (width 0.12))
    (fp_arc (start 0 0.55) (end -2 2.2) (angle -100.5) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 13 VT-read))
    (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_2-G-5,08_1x02_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_D8.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 637052ED)
    (at 205.78 45.72)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 8mm Electrolytic Capacitor")
    (path /63A71318)
    (fp_text reference C5 (at 1.25 -5.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "100µ 35V" (at 1.25 5.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.759698 -2.715) (end -2.759698 -1.915) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.159698 -2.315) (end -2.359698 -2.315) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.331 -0.533) (end 5.331 0.533) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.291 -0.768) (end 5.291 0.768) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.251 -0.948) (end 5.251 0.948) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.211 -1.098) (end 5.211 1.098) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.171 -1.229) (end 5.171 1.229) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.131 -1.346) (end 5.131 1.346) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.091 -1.453) (end 5.091 1.453) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.051 -1.552) (end 5.051 1.552) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.011 -1.645) (end 5.011 1.645) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.971 -1.731) (end 4.971 1.731) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.931 -1.813) (end 4.931 1.813) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.891 -1.89) (end 4.891 1.89) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.851 -1.964) (end 4.851 1.964) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.811 -2.034) (end 4.811 2.034) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.771 -2.102) (end 4.771 2.102) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.731 -2.166) (end 4.731 2.166) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.691 -2.228) (end 4.691 2.228) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.651 -2.287) (end 4.651 2.287) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.611 -2.345) (end 4.611 2.345) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.571 -2.4) (end 4.571 2.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.531 -2.454) (end 4.531 2.454) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.491 -2.505) (end 4.491 2.505) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.451 -2.556) (end 4.451 2.556) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.411 -2.604) (end 4.411 2.604) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.371 -2.651) (end 4.371 2.651) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.331 -2.697) (end 4.331 2.697) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.291 -2.741) (end 4.291 2.741) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.251 -2.784) (end 4.251 2.784) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.211 -2.826) (end 4.211 2.826) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.171 -2.867) (end 4.171 2.867) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.131 -2.907) (end 4.131 2.907) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.091 -2.945) (end 4.091 2.945) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.051 -2.983) (end 4.051 2.983) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.011 -3.019) (end 4.011 3.019) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.971 -3.055) (end 3.971 3.055) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.931 -3.09) (end 3.931 3.09) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.891 -3.124) (end 3.891 3.124) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.851 -3.156) (end 3.851 3.156) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.811 -3.189) (end 3.811 3.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.771 -3.22) (end 3.771 3.22) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.731 -3.25) (end 3.731 3.25) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.691 -3.28) (end 3.691 3.28) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.651 -3.309) (end 3.651 3.309) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.611 -3.338) (end 3.611 3.338) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.571 -3.365) (end 3.571 3.365) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 1.04) (end 3.531 3.392) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 -3.392) (end 3.531 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 1.04) (end 3.491 3.418) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 -3.418) (end 3.491 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 1.04) (end 3.451 3.444) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 -3.444) (end 3.451 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 1.04) (end 3.411 3.469) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 -3.469) (end 3.411 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 1.04) (end 3.371 3.493) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 -3.493) (end 3.371 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 1.04) (end 3.331 3.517) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 -3.517) (end 3.331 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 1.04) (end 3.291 3.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 -3.54) (end 3.291 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 1.04) (end 3.251 3.562) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 -3.562) (end 3.251 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 1.04) (end 3.211 3.584) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 -3.584) (end 3.211 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 1.04) (end 3.171 3.606) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 -3.606) (end 3.171 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 1.04) (end 3.131 3.627) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 -3.627) (end 3.131 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 1.04) (end 3.091 3.647) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 -3.647) (end 3.091 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 1.04) (end 3.051 3.666) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 -3.666) (end 3.051 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 1.04) (end 3.011 3.686) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 -3.686) (end 3.011 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 1.04) (end 2.971 3.704) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 -3.704) (end 2.971 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 1.04) (end 2.931 3.722) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 -3.722) (end 2.931 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 1.04) (end 2.891 3.74) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 -3.74) (end 2.891 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 1.04) (end 2.851 3.757) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 -3.757) (end 2.851 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 1.04) (end 2.811 3.774) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 -3.774) (end 2.811 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 1.04) (end 2.771 3.79) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 -3.79) (end 2.771 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 1.04) (end 2.731 3.805) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 -3.805) (end 2.731 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 1.04) (end 2.691 3.821) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 -3.821) (end 2.691 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 1.04) (end 2.651 3.835) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 -3.835) (end 2.651 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 1.04) (end 2.611 3.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 -3.85) (end 2.611 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 1.04) (end 2.571 3.863) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 -3.863) (end 2.571 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 1.04) (end 2.531 3.877) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 -3.877) (end 2.531 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 1.04) (end 2.491 3.889) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 -3.889) (end 2.491 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 1.04) (end 2.451 3.902) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 -3.902) (end 2.451 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 1.04) (end 2.411 3.914) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 -3.914) (end 2.411 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 1.04) (end 2.371 3.925) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 -3.925) (end 2.371 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 1.04) (end 2.331 3.936) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 -3.936) (end 2.331 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 1.04) (end 2.291 3.947) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 -3.947) (end 2.291 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 1.04) (end 2.251 3.957) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 -3.957) (end 2.251 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 1.04) (end 2.211 3.967) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 -3.967) (end 2.211 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 1.04) (end 2.171 3.976) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 -3.976) (end 2.171 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 1.04) (end 2.131 3.985) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 -3.985) (end 2.131 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 1.04) (end 2.091 3.994) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 -3.994) (end 2.091 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 1.04) (end 2.051 4.002) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 -4.002) (end 2.051 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 1.04) (end 2.011 4.01) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 -4.01) (end 2.011 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 1.04) (end 1.971 4.017) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 -4.017) (end 1.971 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 1.04) (end 1.93 4.024) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 -4.024) (end 1.93 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 1.04) (end 1.89 4.03) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -4.03) (end 1.89 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 1.04) (end 1.85 4.037) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 -4.037) (end 1.85 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 1.04) (end 1.81 4.042) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -4.042) (end 1.81 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 1.04) (end 1.77 4.048) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 -4.048) (end 1.77 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 1.04) (end 1.73 4.052) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 -4.052) (end 1.73 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 1.04) (end 1.69 4.057) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 -4.057) (end 1.69 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 1.04) (end 1.65 4.061) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -4.061) (end 1.65 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 1.04) (end 1.61 4.065) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -4.065) (end 1.61 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 1.04) (end 1.57 4.068) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 -4.068) (end 1.57 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 1.04) (end 1.53 4.071) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 -4.071) (end 1.53 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 1.04) (end 1.49 4.074) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 -4.074) (end 1.49 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -4.076) (end 1.45 4.076) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.41 -4.077) (end 1.41 4.077) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.37 -4.079) (end 1.37 4.079) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -4.08) (end 1.33 4.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.29 -4.08) (end 1.29 4.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.25 -4.08) (end 1.25 4.08) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.776759 -2.1475) (end -1.776759 -1.3475) (layer F.Fab) (width 0.1))
    (fp_line (start -2.176759 -1.7475) (end -1.376759 -1.7475) (layer F.Fab) (width 0.1))
    (fp_circle (center 1.25 0) (end 5.5 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 1.25 0) (end 5.37 0) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 5.25 0) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +24V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_D8.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 63706874)
    (at 187.96 71.12)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 8mm Electrolytic Capacitor")
    (path /638AA834)
    (fp_text reference C4 (at 1.25 -5.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "10µ 16V" (at 1.25 2.54) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 1.25 0) (end 5.25 0) (layer F.Fab) (width 0.1))
    (fp_circle (center 1.25 0) (end 5.37 0) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 5.5 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.176759 -1.7475) (end -1.376759 -1.7475) (layer F.Fab) (width 0.1))
    (fp_line (start -1.776759 -2.1475) (end -1.776759 -1.3475) (layer F.Fab) (width 0.1))
    (fp_line (start 1.25 -4.08) (end 1.25 4.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.29 -4.08) (end 1.29 4.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -4.08) (end 1.33 4.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.37 -4.079) (end 1.37 4.079) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.41 -4.077) (end 1.41 4.077) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -4.076) (end 1.45 4.076) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 -4.074) (end 1.49 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 1.04) (end 1.49 4.074) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 -4.071) (end 1.53 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 1.04) (end 1.53 4.071) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 -4.068) (end 1.57 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 1.04) (end 1.57 4.068) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -4.065) (end 1.61 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 1.04) (end 1.61 4.065) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -4.061) (end 1.65 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 1.04) (end 1.65 4.061) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 -4.057) (end 1.69 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 1.04) (end 1.69 4.057) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 -4.052) (end 1.73 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 1.04) (end 1.73 4.052) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 -4.048) (end 1.77 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 1.04) (end 1.77 4.048) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -4.042) (end 1.81 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 1.04) (end 1.81 4.042) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 -4.037) (end 1.85 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 1.04) (end 1.85 4.037) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -4.03) (end 1.89 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 1.04) (end 1.89 4.03) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 -4.024) (end 1.93 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 1.04) (end 1.93 4.024) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 -4.017) (end 1.971 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 1.04) (end 1.971 4.017) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 -4.01) (end 2.011 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 1.04) (end 2.011 4.01) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 -4.002) (end 2.051 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 1.04) (end 2.051 4.002) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 -3.994) (end 2.091 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 1.04) (end 2.091 3.994) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 -3.985) (end 2.131 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 1.04) (end 2.131 3.985) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 -3.976) (end 2.171 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 1.04) (end 2.171 3.976) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 -3.967) (end 2.211 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 1.04) (end 2.211 3.967) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 -3.957) (end 2.251 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 1.04) (end 2.251 3.957) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 -3.947) (end 2.291 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 1.04) (end 2.291 3.947) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 -3.936) (end 2.331 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 1.04) (end 2.331 3.936) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 -3.925) (end 2.371 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 1.04) (end 2.371 3.925) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 -3.914) (end 2.411 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 1.04) (end 2.411 3.914) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 -3.902) (end 2.451 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 1.04) (end 2.451 3.902) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 -3.889) (end 2.491 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 1.04) (end 2.491 3.889) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 -3.877) (end 2.531 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 1.04) (end 2.531 3.877) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 -3.863) (end 2.571 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 1.04) (end 2.571 3.863) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 -3.85) (end 2.611 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 1.04) (end 2.611 3.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 -3.835) (end 2.651 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 1.04) (end 2.651 3.835) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 -3.821) (end 2.691 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 1.04) (end 2.691 3.821) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 -3.805) (end 2.731 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 1.04) (end 2.731 3.805) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 -3.79) (end 2.771 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 1.04) (end 2.771 3.79) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 -3.774) (end 2.811 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 1.04) (end 2.811 3.774) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 -3.757) (end 2.851 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 1.04) (end 2.851 3.757) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 -3.74) (end 2.891 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 1.04) (end 2.891 3.74) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 -3.722) (end 2.931 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 1.04) (end 2.931 3.722) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 -3.704) (end 2.971 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 1.04) (end 2.971 3.704) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 -3.686) (end 3.011 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 1.04) (end 3.011 3.686) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 -3.666) (end 3.051 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 1.04) (end 3.051 3.666) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 -3.647) (end 3.091 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 1.04) (end 3.091 3.647) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 -3.627) (end 3.131 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 1.04) (end 3.131 3.627) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 -3.606) (end 3.171 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 1.04) (end 3.171 3.606) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 -3.584) (end 3.211 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 1.04) (end 3.211 3.584) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 -3.562) (end 3.251 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 1.04) (end 3.251 3.562) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 -3.54) (end 3.291 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 1.04) (end 3.291 3.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 -3.517) (end 3.331 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 1.04) (end 3.331 3.517) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 -3.493) (end 3.371 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 1.04) (end 3.371 3.493) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 -3.469) (end 3.411 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 1.04) (end 3.411 3.469) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 -3.444) (end 3.451 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 1.04) (end 3.451 3.444) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 -3.418) (end 3.491 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 1.04) (end 3.491 3.418) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 -3.392) (end 3.531 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 1.04) (end 3.531 3.392) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.571 -3.365) (end 3.571 3.365) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.611 -3.338) (end 3.611 3.338) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.651 -3.309) (end 3.651 3.309) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.691 -3.28) (end 3.691 3.28) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.731 -3.25) (end 3.731 3.25) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.771 -3.22) (end 3.771 3.22) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.811 -3.189) (end 3.811 3.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.851 -3.156) (end 3.851 3.156) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.891 -3.124) (end 3.891 3.124) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.931 -3.09) (end 3.931 3.09) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.971 -3.055) (end 3.971 3.055) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.011 -3.019) (end 4.011 3.019) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.051 -2.983) (end 4.051 2.983) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.091 -2.945) (end 4.091 2.945) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.131 -2.907) (end 4.131 2.907) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.171 -2.867) (end 4.171 2.867) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.211 -2.826) (end 4.211 2.826) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.251 -2.784) (end 4.251 2.784) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.291 -2.741) (end 4.291 2.741) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.331 -2.697) (end 4.331 2.697) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.371 -2.651) (end 4.371 2.651) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.411 -2.604) (end 4.411 2.604) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.451 -2.556) (end 4.451 2.556) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.491 -2.505) (end 4.491 2.505) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.531 -2.454) (end 4.531 2.454) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.571 -2.4) (end 4.571 2.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.611 -2.345) (end 4.611 2.345) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.651 -2.287) (end 4.651 2.287) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.691 -2.228) (end 4.691 2.228) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.731 -2.166) (end 4.731 2.166) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.771 -2.102) (end 4.771 2.102) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.811 -2.034) (end 4.811 2.034) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.851 -1.964) (end 4.851 1.964) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.891 -1.89) (end 4.891 1.89) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.931 -1.813) (end 4.931 1.813) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.971 -1.731) (end 4.971 1.731) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.011 -1.645) (end 5.011 1.645) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.051 -1.552) (end 5.051 1.552) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.091 -1.453) (end 5.091 1.453) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.131 -1.346) (end 5.131 1.346) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.171 -1.229) (end 5.171 1.229) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.211 -1.098) (end 5.211 1.098) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.251 -0.948) (end 5.251 0.948) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.291 -0.768) (end 5.291 0.768) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.331 -0.533) (end 5.331 0.533) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.159698 -2.315) (end -2.359698 -2.315) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.759698 -2.715) (end -2.759698 -1.915) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_D8.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 6370519B)
    (at 172.72 48.26 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 8mm Electrolytic Capacitor")
    (path /638A9DC5)
    (fp_text reference C3 (at 1.25 -5.25 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "10µ 16V" (at 2.54 -2.54 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.759698 -2.715) (end -2.759698 -1.915) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.159698 -2.315) (end -2.359698 -2.315) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.331 -0.533) (end 5.331 0.533) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.291 -0.768) (end 5.291 0.768) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.251 -0.948) (end 5.251 0.948) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.211 -1.098) (end 5.211 1.098) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.171 -1.229) (end 5.171 1.229) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.131 -1.346) (end 5.131 1.346) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.091 -1.453) (end 5.091 1.453) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.051 -1.552) (end 5.051 1.552) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.011 -1.645) (end 5.011 1.645) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.971 -1.731) (end 4.971 1.731) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.931 -1.813) (end 4.931 1.813) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.891 -1.89) (end 4.891 1.89) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.851 -1.964) (end 4.851 1.964) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.811 -2.034) (end 4.811 2.034) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.771 -2.102) (end 4.771 2.102) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.731 -2.166) (end 4.731 2.166) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.691 -2.228) (end 4.691 2.228) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.651 -2.287) (end 4.651 2.287) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.611 -2.345) (end 4.611 2.345) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.571 -2.4) (end 4.571 2.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.531 -2.454) (end 4.531 2.454) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.491 -2.505) (end 4.491 2.505) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.451 -2.556) (end 4.451 2.556) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.411 -2.604) (end 4.411 2.604) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.371 -2.651) (end 4.371 2.651) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.331 -2.697) (end 4.331 2.697) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.291 -2.741) (end 4.291 2.741) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.251 -2.784) (end 4.251 2.784) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.211 -2.826) (end 4.211 2.826) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.171 -2.867) (end 4.171 2.867) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.131 -2.907) (end 4.131 2.907) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.091 -2.945) (end 4.091 2.945) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.051 -2.983) (end 4.051 2.983) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.011 -3.019) (end 4.011 3.019) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.971 -3.055) (end 3.971 3.055) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.931 -3.09) (end 3.931 3.09) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.891 -3.124) (end 3.891 3.124) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.851 -3.156) (end 3.851 3.156) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.811 -3.189) (end 3.811 3.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.771 -3.22) (end 3.771 3.22) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.731 -3.25) (end 3.731 3.25) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.691 -3.28) (end 3.691 3.28) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.651 -3.309) (end 3.651 3.309) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.611 -3.338) (end 3.611 3.338) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.571 -3.365) (end 3.571 3.365) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 1.04) (end 3.531 3.392) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 -3.392) (end 3.531 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 1.04) (end 3.491 3.418) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 -3.418) (end 3.491 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 1.04) (end 3.451 3.444) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 -3.444) (end 3.451 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 1.04) (end 3.411 3.469) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 -3.469) (end 3.411 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 1.04) (end 3.371 3.493) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 -3.493) (end 3.371 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 1.04) (end 3.331 3.517) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 -3.517) (end 3.331 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 1.04) (end 3.291 3.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 -3.54) (end 3.291 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 1.04) (end 3.251 3.562) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 -3.562) (end 3.251 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 1.04) (end 3.211 3.584) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 -3.584) (end 3.211 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 1.04) (end 3.171 3.606) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 -3.606) (end 3.171 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 1.04) (end 3.131 3.627) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 -3.627) (end 3.131 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 1.04) (end 3.091 3.647) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 -3.647) (end 3.091 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 1.04) (end 3.051 3.666) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 -3.666) (end 3.051 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 1.04) (end 3.011 3.686) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 -3.686) (end 3.011 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 1.04) (end 2.971 3.704) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 -3.704) (end 2.971 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 1.04) (end 2.931 3.722) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 -3.722) (end 2.931 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 1.04) (end 2.891 3.74) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 -3.74) (end 2.891 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 1.04) (end 2.851 3.757) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 -3.757) (end 2.851 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 1.04) (end 2.811 3.774) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 -3.774) (end 2.811 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 1.04) (end 2.771 3.79) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 -3.79) (end 2.771 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 1.04) (end 2.731 3.805) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 -3.805) (end 2.731 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 1.04) (end 2.691 3.821) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 -3.821) (end 2.691 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 1.04) (end 2.651 3.835) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 -3.835) (end 2.651 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 1.04) (end 2.611 3.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 -3.85) (end 2.611 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 1.04) (end 2.571 3.863) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 -3.863) (end 2.571 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 1.04) (end 2.531 3.877) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 -3.877) (end 2.531 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 1.04) (end 2.491 3.889) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 -3.889) (end 2.491 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 1.04) (end 2.451 3.902) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 -3.902) (end 2.451 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 1.04) (end 2.411 3.914) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 -3.914) (end 2.411 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 1.04) (end 2.371 3.925) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 -3.925) (end 2.371 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 1.04) (end 2.331 3.936) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 -3.936) (end 2.331 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 1.04) (end 2.291 3.947) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 -3.947) (end 2.291 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 1.04) (end 2.251 3.957) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 -3.957) (end 2.251 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 1.04) (end 2.211 3.967) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 -3.967) (end 2.211 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 1.04) (end 2.171 3.976) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 -3.976) (end 2.171 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 1.04) (end 2.131 3.985) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 -3.985) (end 2.131 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 1.04) (end 2.091 3.994) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 -3.994) (end 2.091 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 1.04) (end 2.051 4.002) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 -4.002) (end 2.051 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 1.04) (end 2.011 4.01) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 -4.01) (end 2.011 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 1.04) (end 1.971 4.017) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 -4.017) (end 1.971 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 1.04) (end 1.93 4.024) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 -4.024) (end 1.93 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 1.04) (end 1.89 4.03) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -4.03) (end 1.89 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 1.04) (end 1.85 4.037) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 -4.037) (end 1.85 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 1.04) (end 1.81 4.042) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -4.042) (end 1.81 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 1.04) (end 1.77 4.048) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 -4.048) (end 1.77 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 1.04) (end 1.73 4.052) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 -4.052) (end 1.73 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 1.04) (end 1.69 4.057) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 -4.057) (end 1.69 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 1.04) (end 1.65 4.061) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -4.061) (end 1.65 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 1.04) (end 1.61 4.065) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -4.065) (end 1.61 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 1.04) (end 1.57 4.068) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 -4.068) (end 1.57 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 1.04) (end 1.53 4.071) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 -4.071) (end 1.53 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 1.04) (end 1.49 4.074) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 -4.074) (end 1.49 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -4.076) (end 1.45 4.076) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.41 -4.077) (end 1.41 4.077) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.37 -4.079) (end 1.37 4.079) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -4.08) (end 1.33 4.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.29 -4.08) (end 1.29 4.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.25 -4.08) (end 1.25 4.08) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.776759 -2.1475) (end -1.776759 -1.3475) (layer F.Fab) (width 0.1))
    (fp_line (start -2.176759 -1.7475) (end -1.376759 -1.7475) (layer F.Fab) (width 0.1))
    (fp_circle (center 1.25 0) (end 5.5 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 1.25 0) (end 5.37 0) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 5.25 0) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 154.94 88.9) (end 154.94 35.56) (layer Edge.Cuts) (width 0.05) (tstamp 6371155E))
  (gr_line (start 215.9 35.56) (end 215.9 88.9) (layer Edge.Cuts) (width 0.05) (tstamp 6371155D))
  (gr_line (start 154.94 88.9) (end 215.9 88.9) (layer Edge.Cuts) (width 0.05) (tstamp 6371148E))
  (gr_line (start 215.9 35.56) (end 154.94 35.56) (layer Edge.Cuts) (width 0.05))
  (gr_text "A - C" (at 208.28 93.98) (layer F.Fab) (tstamp 63711488)
    (effects (font (size 1 1) (thickness 0.1)))
  )
  (gr_text "-- ++" (at 187.96 93.98) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.1)))
  )

  (segment (start 165.1 66.04) (end 160.02 66.04) (width 1) (layer B.Cu) (net 1))
  (segment (start 180.3 43.22) (end 180.34 43.18) (width 1) (layer B.Cu) (net 1))
  (segment (start 172.72 45.72) (end 180.3 45.72) (width 1) (layer B.Cu) (net 1))
  (segment (start 180.34 45.72) (end 180.34 43.18) (width 1) (layer B.Cu) (net 1))
  (segment (start 165.1 68.58) (end 165.1 66.04) (width 1) (layer B.Cu) (net 1))
  (segment (start 180.34 68.58) (end 165.1 68.58) (width 1) (layer B.Cu) (net 1))
  (segment (start 195.58 53.34) (end 195.58 50.8) (width 1) (layer B.Cu) (net 1))
  (segment (start 195.58 50.8) (end 187.96 50.8) (width 1) (layer B.Cu) (net 1))
  (segment (start 187.96 50.8) (end 187.96 45.72) (width 1) (layer B.Cu) (net 1))
  (segment (start 187.96 45.72) (end 187.96 40.64) (width 1) (layer B.Cu) (net 1))
  (segment (start 180.34 43.18) (end 180.34 40.64) (width 1) (layer B.Cu) (net 1))
  (segment (start 180.34 40.64) (end 187.96 40.64) (width 1) (layer B.Cu) (net 1))
  (segment (start 195.58 55.88) (end 195.58 53.34) (width 1) (layer B.Cu) (net 1))
  (segment (start 193.04 66.04) (end 193.04 58.42) (width 1) (layer B.Cu) (net 1))
  (segment (start 193.04 58.42) (end 195.58 58.42) (width 1) (layer B.Cu) (net 1))
  (segment (start 195.58 58.42) (end 195.58 55.88) (width 1) (layer B.Cu) (net 1))
  (segment (start 180.34 76.2) (end 180.34 83.82) (width 1) (layer B.Cu) (net 1))
  (segment (start 187.96 53.34) (end 187.96 50.8) (width 1) (layer B.Cu) (net 1))
  (segment (start 193.04 66.04) (end 193.04 73.66) (width 1) (layer B.Cu) (net 1))
  (segment (start 193.04 73.66) (end 180.34 73.66) (width 1) (layer B.Cu) (net 1))
  (segment (start 180.34 73.66) (end 180.34 68.58) (width 1) (layer B.Cu) (net 1))
  (segment (start 180.34 76.2) (end 180.34 73.66) (width 1) (layer B.Cu) (net 1))
  (segment (start 190.46 71.12) (end 193.04 71.12) (width 1) (layer B.Cu) (net 1))
  (segment (start 208.28 40.64) (end 208.28 45.72) (width 1) (layer B.Cu) (net 1))
  (segment (start 187.96 40.64) (end 208.28 40.64) (width 1) (layer B.Cu) (net 1))
  (segment (start 185.42 53.34) (end 185.42 55.88) (width 1) (layer B.Cu) (net 2))
  (segment (start 182.88 55.88) (end 185.42 55.88) (width 1) (layer B.Cu) (net 2))
  (segment (start 182.88 55.88) (end 182.88 58.42) (width 1) (layer B.Cu) (net 2))
  (segment (start 182.88 53.34) (end 182.88 50.8) (width 1) (layer B.Cu) (net 3))
  (segment (start 177.8 50.8) (end 177.8 55.8) (width 1) (layer B.Cu) (net 3))
  (segment (start 177.8 55.8) (end 177.88 55.88) (width 1) (layer B.Cu) (net 3))
  (segment (start 182.88 50.8) (end 177.8 50.8) (width 1) (layer B.Cu) (net 3))
  (segment (start 175.26 60.96) (end 177.8 60.96) (width 1) (layer B.Cu) (net 3))
  (segment (start 177.8 55.96) (end 177.88 55.88) (width 1) (layer B.Cu) (net 3))
  (segment (start 177.8 60.96) (end 177.8 55.96) (width 1) (layer B.Cu) (net 3))
  (segment (start 172.72 58.42) (end 172.72 60.96) (width 1) (layer B.Cu) (net 3))
  (segment (start 172.72 60.96) (end 175.26 60.96) (width 1) (layer B.Cu) (net 3))
  (segment (start 172.72 48.26) (end 185.42 48.26) (width 1) (layer B.Cu) (net 4))
  (segment (start 185.42 48.26) (end 185.42 45.72) (width 1) (layer B.Cu) (net 4))
  (segment (start 165.29 48.26) (end 165.21 48.18) (width 1) (layer B.Cu) (net 4))
  (segment (start 165.29 60.96) (end 165.21 60.88) (width 1) (layer B.Cu) (net 4))
  (segment (start 170.18 60.96) (end 165.29 60.96) (width 1) (layer B.Cu) (net 4))
  (segment (start 170.18 60.96) (end 170.18 48.26) (width 1) (layer B.Cu) (net 4))
  (segment (start 170.18 48.26) (end 165.29 48.26) (width 1) (layer B.Cu) (net 4))
  (segment (start 172.72 48.26) (end 170.18 48.26) (width 1) (layer B.Cu) (net 4))
  (segment (start 190.5 53.34) (end 190.5 63.5) (width 1) (layer B.Cu) (net 5))
  (segment (start 187.96 71.12) (end 187.96 68.58) (width 1) (layer B.Cu) (net 5))
  (segment (start 187.96 68.58) (end 190.5 68.58) (width 1) (layer B.Cu) (net 5))
  (segment (start 190.5 68.58) (end 190.5 63.5) (width 1) (layer B.Cu) (net 5))
  (segment (start 190.5 83.82) (end 195.58 83.82) (width 1) (layer B.Cu) (net 6))
  (segment (start 195.58 83.82) (end 195.58 78.74) (width 1) (layer B.Cu) (net 6))
  (segment (start 205.74 78.74) (end 205.74 83.82) (width 1) (layer B.Cu) (net 6))
  (segment (start 205.74 71.12) (end 205.74 78.74) (width 1) (layer B.Cu) (net 6))
  (segment (start 203.2 78.74) (end 205.74 78.74) (width 1) (layer B.Cu) (net 6))
  (segment (start 195.58 78.74) (end 203.2 78.74) (width 1) (layer B.Cu) (net 6))
  (segment (start 205.74 71.12) (end 203.2 71.12) (width 1) (layer B.Cu) (net 6))
  (segment (start 205.74 53.34) (end 205.74 71.12) (width 1) (layer B.Cu) (net 6))
  (segment (start 210.82 53.34) (end 205.74 53.34) (width 1) (layer B.Cu) (net 6))
  (segment (start 205.74 48.26) (end 205.74 53.34) (width 1) (layer B.Cu) (net 6))
  (segment (start 190.5 43.18) (end 205.74 43.18) (width 1) (layer B.Cu) (net 6))
  (segment (start 205.74 43.18) (end 205.74 48.26) (width 1) (layer B.Cu) (net 6))
  (segment (start 190.5 45.72) (end 190.5 43.18) (width 1) (layer B.Cu) (net 6))
  (segment (start 185.42 83.82) (end 185.42 76.2) (width 1) (layer B.Cu) (net 7))
  (segment (start 203.2 60.96) (end 203.2 45.72) (width 1) (layer B.Cu) (net 7))
  (segment (start 203.2 45.72) (end 195.58 45.72) (width 1) (layer B.Cu) (net 7))
  (segment (start 208.28 58.42) (end 208.28 60.96) (width 1) (layer B.Cu) (net 7))
  (segment (start 208.28 60.96) (end 210.82 60.96) (width 1) (layer B.Cu) (net 7))
  (via (at 203.2 60.96) (size 2) (drill 1) (layers F.Cu B.Cu) (net 7))
  (segment (start 198.12 60.96) (end 203.2 60.96) (width 1) (layer B.Cu) (net 7))
  (via (at 208.28 60.96) (size 2) (drill 1) (layers F.Cu B.Cu) (net 7))
  (segment (start 203.2 60.96) (end 208.28 60.96) (width 1) (layer F.Cu) (net 7))
  (segment (start 185.42 76.2) (end 198.12 76.2) (width 1) (layer B.Cu) (net 7))
  (segment (start 195.58 71.12) (end 198.2 71.12) (width 1) (layer B.Cu) (net 7))
  (segment (start 195.58 71.12) (end 195.58 66.04) (width 1) (layer B.Cu) (net 7))
  (segment (start 198.12 76.2) (end 198.12 60.96) (width 1) (layer B.Cu) (net 7))
  (segment (start 210.82 83.82) (end 210.82 76.2) (width 1) (layer B.Cu) (net 8))
  (segment (start 208.28 55.88) (end 210.82 55.88) (width 1) (layer B.Cu) (net 9))
  (segment (start 157.48 66.04) (end 157.48 38.1) (width 1) (layer B.Cu) (net 10))
  (segment (start 162.63 38.1) (end 162.71 38.18) (width 1) (layer B.Cu) (net 10))
  (segment (start 157.48 38.1) (end 162.63 38.1) (width 1) (layer B.Cu) (net 10))
  (segment (start 160.21 48.18) (end 157.56 48.18) (width 1) (layer B.Cu) (net 10))
  (segment (start 167.64 66.04) (end 167.64 63.5) (width 1) (layer B.Cu) (net 11))
  (segment (start 167.64 63.5) (end 160.02 63.5) (width 1) (layer B.Cu) (net 11))
  (segment (start 160.02 63.5) (end 160.02 50.8) (width 1) (layer B.Cu) (net 11))
  (segment (start 162.63 50.8) (end 162.71 50.88) (width 1) (layer B.Cu) (net 11))
  (segment (start 160.02 50.8) (end 162.63 50.8) (width 1) (layer B.Cu) (net 11))
  (segment (start 182.88 43.18) (end 182.88 45.72) (width 1) (layer B.Cu) (net 12))
  (segment (start 175.26 83.82) (end 175.26 71.12) (width 1) (layer B.Cu) (net 13))
  (segment (start 170.18 71.12) (end 172.72 71.12) (width 1) (layer B.Cu) (net 13))
  (segment (start 172.72 71.12) (end 175.26 71.12) (width 1) (layer B.Cu) (net 13))
  (segment (start 165.1 76.2) (end 167.64 76.2) (width 1) (layer B.Cu) (net 14))
  (segment (start 170.18 78.74) (end 170.18 83.82) (width 1) (layer B.Cu) (net 14))
  (segment (start 170.18 76.2) (end 170.18 78.74) (width 1) (layer B.Cu) (net 14))
  (segment (start 167.64 76.2) (end 170.18 76.2) (width 1) (layer B.Cu) (net 14))
  (segment (start 165.1 78.74) (end 165.1 83.82) (width 1) (layer B.Cu) (net 15))
  (segment (start 162.56 78.74) (end 165.1 78.74) (width 1) (layer B.Cu) (net 15))
  (segment (start 162.56 73.66) (end 162.56 78.74) (width 1) (layer B.Cu) (net 15))
  (segment (start 172.72 73.66) (end 162.56 73.66) (width 1) (layer B.Cu) (net 15))
  (segment (start 160.02 83.82) (end 160.02 76.2) (width 1) (layer B.Cu) (net 16))
  (segment (start 160.02 76.2) (end 157.48 76.2) (width 1) (layer B.Cu) (net 16))
  (segment (start 200.66 86.36) (end 213.36 86.36) (width 1) (layer B.Cu) (net 17))
  (segment (start 213.36 58.42) (end 210.82 58.42) (width 1) (layer B.Cu) (net 17))
  (segment (start 210.82 66.04) (end 213.36 66.04) (width 1) (layer B.Cu) (net 17))
  (segment (start 213.36 66.04) (end 213.36 58.42) (width 1) (layer B.Cu) (net 17))
  (segment (start 200.66 83.82) (end 200.66 86.36) (width 1) (layer B.Cu) (net 17))
  (segment (start 213.36 86.36) (end 213.36 66.04) (width 1) (layer B.Cu) (net 17))
  (segment (start 172.72 63.5) (end 180.34 63.5) (width 1) (layer B.Cu) (net 18))
  (segment (start 180.34 63.5) (end 180.34 53.34) (width 1) (layer B.Cu) (net 18))
  (segment (start 185.42 63.5) (end 185.42 66.04) (width 1) (layer B.Cu) (net 18))
  (segment (start 180.34 63.5) (end 185.42 63.5) (width 1) (layer B.Cu) (net 18))
  (segment (start 193.04 55.88) (end 193.04 53.34) (width 1) (layer B.Cu) (net 19))
  (segment (start 200.66 53.34) (end 198.12 53.34) (width 1) (layer B.Cu) (net 20))
  (segment (start 193.04 48.26) (end 193.04 45.72) (width 1) (layer B.Cu) (net 20))
  (segment (start 198.12 48.26) (end 193.04 48.26) (width 1) (layer B.Cu) (net 20))
  (segment (start 198.12 58.42) (end 198.12 48.26) (width 1) (layer B.Cu) (net 20))

)
